1. **General**
	1. **Summary**
		1. Related Documents
			1. Drawings and general provisions of the Subcontract apply to this Section.
			2. Review these documents for coordination with additional requirements and information that apply to the work under this section.
		2. Section Includes
			1. Coupling
	2. **References**
		1. General
			1. The following documents form part of the Specifications to the extent stated. Where differences exist between codes and standards, the one affording the greatest protection shall apply.
			2. Unless otherwise noted, the referenced standard edition is the current one at the time of commencement of the Work.
			3. Refer to Division 01 Section "General Requirements" for the list of applicable regulatory requirements.
	3. **Submittals**
		1. Submit shop drawings/product data sheets for all products specified in Part 2 of this Section.
	4. **Quality Assurance**
		1. All materials shall meet or exceed all applicable referenced standards, federal, state and local requirements, and conform to codes and ordinances of authorities having jurisdiction.
2. **Products**
	1. **Coupling**
		* 1. Coupling
				1. Shielded Regular Duty No Hub coupling, 1-1/2" to 12” Pipe Size to connect cast iron pipe. Type 301 AISI Stainless Steel Clamps, Neoprene Gasket tested and certified to ASTM C-564, Type 305 AISI Stainless Steel 5/16" hex head screws, Type 304 AISI Stainless Steel screw housing, Type 301 AISI Stainless Steel Eyelets. Tested and Certified to the ASTM C1277-2009a, CISPI 310-2010 and NSF Standards and listed with I.A.P.M.O.
				2. Basis of Design:

MIFAB MI-QHUB

1. **Execution**
	1. **Demolition**
		1. Refer to demolition requirements specified in Section entitled Demolition and Revision Work.
	2. **Installation**
		1. Installed in accordance with manufacturer’s instructions.

**End of Section**