* 1. FLOOR SINKS

\*\* NOTE TO SPECIFIER \*\* Delete paragraphs not required.

* + 1. PVC Floor Sinks PVC Floor Sinks

\*\* NOTE TO SPECIFIER \*\* PVC floor sinks are manufactured out of PVC material to provide the ultimate in sanitary design. PVC material has excellent resistance to chemicals such as the acids contained in fruits, vegetables, and fats. The smooth, uniform surface is easy to clean, and the floor sink will not chip or rust. PVC floor sinks are lightweight for easier handling, installation, and transportation.

* + - 1. Attributes: For use in kitchens, restaurants, grocery stores, hospitals, schools, and other areas that require a medium volume sanitary drain. The light duty grate is recommended for foot traffic. The PVC light duty grate is not recommended for vehicle traffic.
				1. Product: FS520-30 Deep PVC Floor Sink: 8 inch square by 6 inches deep. Available with optional dome bottom strainer and with full, three-quarter, or half PVC, nickel bronze or stainless steel grate configurations. Sizes: 2, 3, and 4 inch. Outlet Socket: 4 inch connection body fits into 4 inch PVC pipe and over 3 inch PVC pipe.
		1. Rectangular Floor Sinks:
			1. Attributes: Used in kitchens, restaurants, grocery stores, hospitals, schools, and other areas requiring a small volume sanitary drain. The light duty grate is not suitable for foot traffic. Regular top is for installation under counters and along walls.

\*\* NOTE TO SPECIFIER \*\* Delete product options not required.

* + - * 1. Product: FS1530 Floor Area and Indirect Sanitary Waste Drain 8 x 4 x 4 inches: Deep cast iron floor area and indirect sanitary waste drain with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1530-FL Floor Area and Indirect Sanitary Waste Drain 8 x 4 x 4 inch: Deep cast iron floor area and indirect sanitary waste drain with white acid resistant porcelain enamel coated interior and loose set grate and Anti-splash aluminum dome strainer included. Anchor flange with weepholes engineered to receive water proofing membrane. Membrane clamps are recommended for use with anchor flange. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
		1. Round Floor Sinks:

\*\* NOTE TO SPECIFIER \*\* Delete attributes and product options not required.

* + - 1. Attributes: Used in kitchens, restaurants, grocery stores, hospitals, schools, and other areas that require a small volume sanitary drain. The light duty grate is not recommended for foot traffic.
				1. Product: FS1750 Floor Area and Indirect Sanitary Waste Drain: 8 inch Round x 6 inch deep cast iron floor area and indirect sanitary waste drain with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.

Product: FS1750-FL Floor Area and Indirect Sanitary Waste Drain Anchor Flange: 8 inch Round x 6 inch deep cast iron floor area and indirect sanitary waste drain with white acid resistant porcelain enamel coated interior, loose set grate and anchor flange with weepholes. Anti-splash aluminum dome strainer included. Anchor flange is engineered to receive water proofing membrane. Membrane clamps are recommended for use with the anchor flange. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas

* + - * 1. Product: FS1760 Floor Area and Indirect Sanitary Waste Drain: 12 inch round x 8 inch deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1760-FL Floor Area & Indirect Sanitary Waste Drain with Anchor Flange: 12 inch Round x 8 inch deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior, loose set grate and anchor flange with weepholes. Anti-splash aluminum dome strainer included. Anchor flange is engineered to receive water proofing membrane. Membrane clamps are recommended for use with the anchor flange. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
			1. Attributes: Used in areas that require a sanitary coated, shallow body for indirect waste applications.
				1. Product: FS1950 Shallow Floor Sink: 9 inch round, shallow, cast iron floor sink with acid resistant electrostatically applied epoxy coated body, grate, and integral sediment bucket. Pipe Sizes: 2,3, 4, 5, and 6 inch.
		1. Square Floor Sinks

\*\* NOTE TO SPECIFIER \*\* Delete attributes and product options not required.

* + - 1. Attributes: Used in kitchens, restaurants, grocery stores, hospitals, schools, and other areas that require a medium volume sanitary drain. The light duty grate is not recommended for foot traffic.
				1. Product: FS1520 Floor Area and Indirect Sanitary Waste Drain. 8 x 8 x 6" deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1520-FL Floor Area and Indirect Sanitary Waste Drain 8 x 8 x 6" with Anchor Flange. Deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate and anchor flange with weepholes. Anti-splash aluminum dome strainer included. Anchor flange is engineered to receive water proofing membrane. Membrane clamps are recommended for use with the anchor flange. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
			2. Attributes: Used in kitchens, restaurants, grocery stores, hospitals, schools, and other areas that require a large volume sanitary drain. The light duty grate is not recommended for foot traffic.
				1. Product: FS1720 Floor Area and Indirect Sanitary Waste Drain: 12 x 12 x 6" deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1720-FL Floor Area and Indirect Sanitary Waste Drain 12 x 12 x 6" with Anchor Flange: Deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Anchor flange is engineered to receive water proofing membrane. Membrane clamps are recommended for use with the anchor flange. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
				3. Product: FS1730 Floor Area and Indirect Sanitary Waste Drain. 12 x 12 x 8 inch deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				4. Product: FS1730-FL Floor Area and Indirect Sanitary Waste Drain 12 x 12 x 8" with Anchor Flange: Deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior, loose set grate and anchor flange with weepholes. Membrane clamps are recommended for use with the anchor flange. Anti-splash aluminum dome strainer included. Specify -3 stainless steel frame and grate for decorative areas.
				5. Product: FS1740 Floor Area and Indirect Sanitary Waste Drain. 12 x 12 x 10"
				6. deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior and loose set grate. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				7. Product: FS1740-FL Floor Area and Indirect Sanitary Waste Drain 12 x 12 x 10" with Anchor Flange: Deep cast iron floor area and indirect sanitary waste drain complete with white acid resistant porcelain enamel coated interior, loose set grate and anchor flange with weepholes. Membrane clamps are recommended for use with the anchor flange. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
				8. Product: FS1770 Deep Floor Area and Indirect Sanitary Waste Drain: 16 x 16 x 9 inch deep floor area and indirect sanitary waste drain complete with white acid resistant coated steel interior and heavy duty ductile iron loose set grate with white acid resistant coating. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
				9. Product: FS1770-FL Floor Area and Indirect Sanitary Waste Drain 16 x 16 x 9" with Anchor Flange: Deep floor area and indirect sanitary waste drain complete with white acid resistant coated steel interior and heavy duty ductile iron loose set grate with white acid resistant coating and anchor flange. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch. Specify -3 stainless steel frame and grate for decorative areas.
				10. Product: FS1790 - 24 x 24 x 17" Deep Floor Sink with Anchor Flange: Deep floor area and indirect sanitary waste drain complete with white acid resistant coated steel interior and heavy duty fabricated steel loose set grate with white acid resistant coating and anchor flange. Anti-splash aluminum dome strainer included. Pipe Sizes: 2,3, and 4 inch.
		1. Stainless steel floor sinks
			1. Attributes: Used in kitchens, restaurants, breweries, dairies, creameries, food processing locations, nuclear, gas and coal fired power stations, chemical plants, laboratories, and other areas where the corrosion resistance of Type 304 stainless steel is required for superior sanitation. Anchor flange is designed to receive water proofing membrane. A membrane clamp is recommended to secure the water proofing membrane to the anchor flange.

\*\* NOTE TO SPECIFIER \*\* Delete product options not required.

* + - * 1. Product: FS1910-FL Floor Area and Indirect Sanitary Waste Drain 12 x 12 x 4" with Anchor Flange: 16 gauge, Type 304 stainless steel sanitary floor area and indirect waste drain complete with cast stainless steel secured rim and grate with allen key vandal proof stainless steel screws, stainless steel anchor flange with weepholes and anti-splash dome strainer. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1920-FL Floor Area and Indirect Sanitary Waste Drain 12 x 12 x 6” with Anchor Flange: 16 gauge, Type 304 stainless steel sanitary floor area and indirect waste drain complete with cast stainless steel secured rim and grate with allen key vandal proof stainless steel screws, stainless steel anchor flange with weepholes and anti-splash dome strainer. Pipe Sizes: 2,3, and 4 inch.
				3. Product: FS1930-FL Floor Area & Indirect Sanitary Waste Drain 12 x 12 x 8" with Anchor Flange: 16 gauge, Type 304 stainless steel sanitary floor area and indirect waste drain complete with cast stainless steel secured rim and grate with allen key vandal proof stainless steel screws, stainless steel anchor flange with weepholes and anti-splash dome strainer. Pipe Sizes: 2,3, and 4 inch.
				4. Product: FS1940-FL Floor Area & Indirect Sanitary Waste Drain 12 x 12 x 10" with Anchor Flange: 16 gauge, Type 304 stainless steel sanitary floor area and indirect waste drain complete with cast stainless steel secured rim and grate with allen key vandal proof stainless steel screws, stainless steel anchor flange with weepholes and anti-splash dome strainer. Pipe Sizes: 2,3, and 4 inch.
		1. Other Floor Sinks Other Floor Sinks

\*\* NOTE TO SPECIFIER \*\* Delete attributes and product options not required.

* + - 1. Attributes: Used in areas to support floor sinks off the structural slab.
				1. Product: FS1959 Floor Sink Installation Stabilization Plate: 8 x 8 inch, 16 gauge, steel, electrostatically applied powder epoxy coated floor sink installation stabilization plate. 12-1/2 inch square and 1-1/2 inch high. Complete with four 5/16 inch all threaded rods and adjustable knock outs to accommodate 3 and 4 inch outlet connections. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1960 Floor Sink Installation Stabilization Plate: 12 x 12 inch, 16 gauge, steel, electrostatically applied powder epoxy coated floor sink installation stabilization plate. 14-1/2 inch square and 1-1/2 inch high. Complete with four 5/16 inch all threaded rods and adjustable knock outs to accommodate 3 and 4 inch outlet connections. Pipe Sizes: 2,3, and 4 inch.
			2. Attributes: Used in areas where porcelain enamel floor sink has chipped and / or worn off from already installed floor sinks. The stainless steel liner is inserted into existing porcelain enamel floor sink.
				1. Product: FS1970 Replacement Floor Sink Liner 8 x 8 x 6 inches. 16 gauge stainless steel, type 304 floor sink replacement liner with internal dome strainer. External pipe gasket seal and light duty slotted loose set stainless steel grate. Pipe Sizes: 2,3, and 4 inch.
				2. Product: FS1980 Replacement Floor Sink Liner 12 x 12 x 6 inches. 16 gauge stainless steel, type 304 floor sink replacement liner with internal dome strainer. External pipe gasket seal and light duty slotted loose set stainless steel grate. Pipe Sizes: 2,3, and 4 inch.
				3. Product: FS1990 Replacement Floor Sink Liner 12 x 12 x 8 inches. 16 gauge, stainless steel, type 304 floor sink replacement liner with internal dome strainer. External pipe gasket seal and light duty slotted loose set stainless steel grate. Pipe Sizes: 2,3, and 4 inch.
				4. FS2000 Replacement Floor Sink Liner 12 x 12 x 10 inches. 16 gauge, stainless steel, type 304 floor sink replacement liner with internal dome strainer. External pipe gasket seal and light duty slotted loose set stainless steel grate. Pipe Sizes: 2,3, and 4 inch.